Bungee-CL PX4 Opto Driver 
for
Sapera LT Imaging Library 
for
Windows XP / Vista / Windows 7
 (32-64 Bits)
Version 1.00.01.20010
par Teledyne DALSA Inc., August 13th, 2015
				
Table of Contents

•	Installation Notes
•	Disk Contents
•	Hardware Supported
•	New Features
·	Backward Compatibility
·	Known Limitations
·	Known Issues

Installation Notes

	Please consult the Bungee-CL PX4 Opto User's manual for detailed installation procedure for the supported Operating Systems.

Disk Contents

	Install root dir

		readme.txt
	\Bin
		CorDeviceManager program
	
	\Firmware
		Firmware

	\Help
		Bungee -CL PX4 Opto Manual in Help format        
		Bungee -CL PX4 Opto Manual in PDF format 

	\Inf	
		Windows Plug & Play driver files

	Windows system directory (winnt\system32)                       
		Dynamic Link Libraries (DLL's) 

	Windows driver directory (winnt\system32\drivers)       
		Device driver files   

	Windows inf directory (winnt\inf)
		Device driver information file  

Hardware Supported

·	Bungee -CL PX4 Opto (with 1024MB of on-board memory)

Backward Compatibility
·	Compatible with Sapera LT version 7.10 and later.

New Features

·	Key Features for X64 Xcelera-CL PX4 FULL
·	Windows XP / VISTA / Windows 7, 32-64 Bits
·	1 Base Camera Link cameras
·	Linescan & areascan (progressive) Camera Link cameras
·	Monochrome 8, 10, and 12 bits per pixel, color 8
·	Up to 3 taps
·	On-board serial port accessible as a standard PC COM port
·	Shaft encoder support
·	Trigger input 
·	Internal frame trigger
·	Strobe
·	Input LUTs
Mono: 256x8-bit, 1024x10-bit, 1024x8-bit, 4096x12-bit, 4096x10-bit, 4096x8-bit
Color: 3x256x8-bit (Base)
·	Time Slot (Time Multiplexing)
·	Flat Field Correction
·	Bayer Decoding
·	Frame Integration

Added

Fixes

Notes

·	Compatible with Sapera LT version 7.10 and later.
·	Cropping width must be a multiple of 16 pixels.
·	Hactive must be a multiple of 16 pixels/Taps with multi-tap camera
·	After a logoff, the user must reboot the system if he wants to use the serial port.
·	When windows prompt "Find new hardware Bungee-CL PX4 Opto board", the user must reboot the system in order to use the serial port.
·	External Trigger Acquisition Callback 
Line scan: edge and level trigger
Area scan: edge trigger only
·	The LUT must not be change/set while grabbing.
•	Horizontal flip is not support for dual channel camera and for 2 alternated taps 10 or 12 bits camera.
•	In variable frame length, the external trigger must be inactive for at least one line.