X64-CL CZM Driver
for Sapera LT Imaging Library
Windows XP / Vista / 7 (32/64)
Version History
Teledyne DALSA Inc.

Version 1.00.01.3010 
July 12th, 2012

Key Features

·	Key Features for X64-CL CZM
·	Windows 2000/XP
·	2 Base or 1 Medium Camera Link cameras
·	Linescan & areascan (progressive) Camera Link cameras
·	Monochrome 8, 10, and 12 bits per pixel, color 8, 10 or 12 bits per pixels with a output of 8 or 10 bits 
·	Up to 4 taps
·	On-board serial port accessible as a standard PC COM port
·	Shaft encoder support
·	Trigger input 
·	Internal frame trigger
·	Strobe
·	Input LUTs
Mono: 256x8-bit, 1024x10-bit, 1024x8-bit, 4096x12-bit, 4096x10-bit, 4096x8-bit Input LUTs per tap
Color: 3x256x8-bit (Base), 3x1024x10-bit or 3x4096x12-bit (Medium)
·	Time Slot (Time Multiplexing)
·	Flat Field Correction
·	Bayer Decoding
·	Frame Integration

·	Key Features for X64-CL CZM\Lite
·	Windows 2000/XP
·	1 Base Camera Link camera
·	Linescan & areascan (progressive) Camera Link cameras
·	Monochrome 8, 10, and 12 bits per pixel, color 8 bits per pixels
·	On-board serial port accessible as a standard PC COM port
·	Shaft encoder support
·	Trigger input 
·	Internal frame trigger
·	Strobe
·	Input LUTs
Mono: 256x8-bit, 1024x10-bit, 1024x8-bit, 4096x12-bit, 4096x10-bit, 4096x8-bit Input LUTs per tap
Color: 3x256x8-bit
·	Frame Integration
·	Bayer with Flatfield correction

New Features

·	Added support for line integration with double pulse (CMI #240)

Fixes

Backward Compatibility

·	Compatible with Sapera LT version 5.20 and later (XP only)

Notes

·	Compatible with Sapera LT version 5.20 and later.
·	Cropping width must be a multiple of 8 pixels.
·	Hactive must be a multiple of 8 pixels/Taps with multi-tap camera
·	Multi-board System: All X64-CL CZM boards must have the same configuration (2 Base or 1 Medium)
·	After a logoff, the user must reboot the system if he wants to use the serial port.
·	When windows prompt "Find new hardware X64-CL CZM board", the user must reboot the system in order to use the serial port.
·	4 taps of 8 bits with alternated taps and cameralink configuration "two bases" is not supported.
·	External Trigger Acquisition Callback 
Line scan: edge and level trigger
Area scan: edge trigger only

=============================================
Previous Versions	
See Internal_History.txt (internal only).